**RFA 9.5mT (405KHz) 5W description:**

Vds = 30V

Vgs = 5.5V

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Voltage (p-p)** | **Current (p-p)** | **Power** |
| **Input** | 1.424V | 7mA | 0.1mW |
| **First stage** | 2V | 19.2A | 64mW |
| **Second stage** | 44.9V | 0.9A | 5.1W |